{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["第十五届全运会花样游泳器材配置清单"],"read":"whole","date_system":"1900"}

{"sheet":"第十五届全运会花样游泳器材配置清单","index":0,"n_rows":122,"n_cols":6,"rows_kept":122,"merged":[[0,0,0,5],[1,0,1,4],[2,0,2,4],[3,0,4,0],[3,1,4,1],[3,2,4,2],[3,3,4,3],[3,4,4,4],[3,5,4,5],[14,0,14,4],[15,0,16,0],[15,1,16,1],[15,2,16,2],[15,3,16,3],[15,4,16,4],[15,5,16,5],[26,0,26,4],[27,0,28,0],[27,1,28,1],[27,2,28,2],[27,3,28,3],[27,4,28,4],[27,5,28,5],[41,0,41,4],[42,0,43,0],[42,1,43,1],[42,2,43,2],[42,3,43,3],[42,4,43,4],[42,5,43,5],[53,0,53,4],[54,0,55,0],[54,1,55,1],[54,2,55,2],[54,3,55,3],[54,4,55,4],[54,5,55,5]]}
["第十五届全运会花样游泳项目竞赛器材配置清单                                                                                   比赛场馆：江门体育中心游泳馆 "]
["一、竞赛专用器材"]
["1、水下音响系统技术要求和设备清单"]
["序号","器材名称","功能与规格及说明","单位","数量","形式"]
[]
[1,"控制主机","技术要求：1、CPU：I7\n2、内存容量：12GB\n3、硬盘：512G","套",1,"租赁"]
[2,"数字调音台","技术要求：1、频率响应 话筒/线路输入到任何输出端 20Hz-20kHz ±0.5dB\n2、总谐波失真和噪声 -30dBu 输入到混音，话筒增益40dB<0.007%\n3、频率响应 20Hz22kHz±0.25dB \n4、失真度 <0.008%@1kHz+12dBu \n5、采样频率 96kHz\n6、系统延时 <1.4mS","台",1,"租赁"]
[3,"音频控制软件","技术要求：1、录制和储存音频数据\n2、监听水下声音\n3、测试声音分贝大小\n4、显示音频波形、频率","套",1,"租赁"]
[4,"外置声卡","技术要求：1、放大音频信号\n2、接收下水音频\n3、处理和过滤音频信号","套",1,"租赁"]
[5,"功放（水下音箱）","技术要求：1、额定输出：2500W\n2、输入灵敏度：0dBV\n3、信噪比>90dB","台",2,"租赁"]
[6,"水下扬声器","技术要求：1、高级别的压电弯曲盘技术\n2、材料：PVC和环氧树脂\n3、抗盐性，不会出现电化学腐蚀，非磁性材料组成\n4、高效的声功率\n5、深度能力：45m\n6、尺寸： 21.6cm直径 5.1cm轴向长度\n7、重量：2.0千克\n8、提供7.62米长的线缆\n9、输入电流最大200瓦特\n10、输入阻抗4000 ohms\n11、频率200 Hz 到 32 KHz。也可在某个方向上达到更大频率\n12、单向波束图型在2 KHz\n13、用于花样游泳水下音乐播放","只",8,"租赁"]
[7,"转换器","技术要求：电压≥25V","只",8,"租赁"]
[8,"水听器","技术要求：1、监听水下音频信号\n2、波束宽:+/-2dB,全向性\n3、最小距离:100m\n4、最小水深:5m","只",2,"租赁"]
[]
["2、岸上音响系统技术要求和设备清单"]
["序号","器材名称","功能与规格及说明","单位","数量","形式"]
[]
[1,"笔记本电脑","技术要求：1、CPU：i7\n2、内存容量：8GB\n3、硬盘：512G\n4、屏幕尺寸：15英寸\n5、带光驱，可读取CD文件","台",2,"租赁"]
[2,"无线麦克风","技术要求：1、射频稳定度：±0.005%(-10-50℃) \n2、载波频段：UHF 500-950MHz（标准：630-790MHz）","个",4,"租赁"]
[3,"有线鹅颈话筒","技术要求：1、频率响应：30-18,000Hz\n2、高通滤波：80Hz,18dB/octave\n3、进口话筒信噪比高，噪声少 声音清晰","个",3,"租赁"]
[4,"功放（水上主扩音箱）","技术要求：1、输出功率：8欧 - 2X1200；4欧 - 2X1700W\n2、频率响应+0/-3 dB：20 Hz - 20 kHz   （1瓦 8欧）\n3、信噪比：>100 dBA","台",2,"租赁"]
[5,"功放（水上返听音箱）","技术要求：1、输出功率：8欧 - 2X1200W；4欧 - 2X1500W\n2、频率响应+0/-3 dB：20 Hz - 20 kHz （1瓦 8欧）\n3、信噪比：>100 dBA","台",1,"租赁"]
[6,"水上音箱","技术要求：1、频率响应：40Hz-20kHz±3dB\n2、额定功率：1000W 峰值1200W\n3、灵敏度：110dB\n4、最大声压级：136dB \n5、标准阻抗：8Ω\n6、尺寸(mm)：675×434×368\n7、净重(kg)：30\n8、进口音箱一致性好干涉少，相比较国产的，进口音箱的声音音质更高","个",6,"租赁"]
[7,"返送音箱","技术要求：1、频率响应：45Hz-20kHz±3dB\n2、额定功率：850W\n3、灵敏度：101dB\n4、最大声压级：130dB \n5、标准阻抗：8 Ω\n6、尺寸(mm)：260×349×546(WxDxH)\n7、净重(kg)：15\n8、进口音箱一致性好干涉少，相比较国产的，进口音箱的声音音质更高","个",2,"租赁"]
[8,"分贝仪","比赛用","个",1,"租赁"]
[]
["3、水下仲裁回放系统技术要求和设备清单"]
["序号","设备名称","功能、规格、说明","单位","数量","形式"]
[]
[1,"云台摄像机","技术要求：\n图像传感器：1/2.5型4K MOS\n视像分辨率：3480*2160\n变焦倍数：24倍光学变焦\n视频输出接口：HDMI，12G-SDI，3G-SDI\n网络接口：LAN\n控制接口：RS-422\n输出格式：[4K 格式] 2160/59.94p，2160/50p，2160/29.97p (原生)，2160/25p (原生)，2160/24p (原生)，2160/23.98p (原生)[HD 格式] 1080/59.94p，1080/50p，1080/29.97p (原生)，1080/29.97PsF，1080/25p (原生)，1080/25PsF，1080/23.98p 或 59.94i，1080/24p (原生)，1080/23.98p (原生)，1080/23.98PsF，1080/59.94i，1080/50i，720/59.94p，720/50p\n水平旋转范围：±175°\n俯仰范围：-30°至210°\n视频压缩格式：JPEG(MJPEG)，H.264，H.265，NDI|HX，高带宽NDI\nNDI支持：NDI，NDI|HX：作为标准包括在内\n机械水平旋转/俯仰：直接驱动系统\n摄像系统、镜头和云台一体化设计在一小巧轻盈的机身中。","台",3,"租赁"]
[2,"控制系统","技术要求：通过IP和串行控制功能Conventional实现简单的连接和操控\n连接AW-HS50到IP控制，实现高效自由操作\n支持串行控制\n摄像机遥控器协议×4，RS422 (Panasonic AW 系列协议)连接串行 : zui多5台摄像机\nIP : zui多95台摄像机调整功能水平/俯仰，变焦， 聚焦，\n光圈，增益底电平，快门，细节调整，白平衡，\n(自动， R/B 增益)，黑平衡，\n(自动， R/B 基准)，切换场景文件切换台控制连接IP: 1支持的切换台AW-HS50联动装置摄像机状态显示,Tally接收,\n切换台母线选择(AUX/PVW/PinP/KEY-F),\n操纵杆 (水平/俯仰,PinP位置)接口LAN10BASE-T/100BASE-TX ( IP 协议)：RJ45 x 1\n TO PAN/TILT HEADRS422 (串行控制协议)：RJ45 x 5TALLY/GPITALLY 输入 x 5 通道\nGPI 输入 x 4 通道\nGPI 输出 x 4 通道\nD-sub 15 pin(母) x 1","套",3,"租赁"]
[3,"适配器","技术要求：专用电源适配器","个",3,"租赁"]
[4,"交换机","技术要求：应用层级：二层\n传输速率：10/100Mbps\n交换方式：存储-转发\n背板带宽：1Gbps","台",1,"租赁"]
[5,"防水套件","技术要求：防水、防氯、防腐蚀，高透光性，防水深度达20米","件",3,"租赁"]
[6,"防护罩","技术要求：保护防水罩，防止划伤","件",3,"租赁"]
[7,"水下摄像机复合缆","\n技术要求：60米长，供电，控制，信号传输","条",3,"租赁"]
[8,"采集卡","技术要求：DeckLink专门为处理非常高品质的视频所设计的，支持采集Apple ProRes、DNxHD或甚至10bit无压缩等常见视频格式，支持525i、625i、720p、1080i和1080p视频格式，上至1080p60。","个",6,"租赁"]
[9,"采集回放终端","技术要求：采集、储存、回放等","个",6,"租赁"]
[10,"PAD","技术要求：128G内存 11英寸","个",6,"租赁"]
[11,"PAD支架","技术要求：稳固型","个",6,"租赁"]
[]
["4、计时记分系统技术要求和设备清单"]
["序号","器材名称","功能与规格及说明","单位","数量","形式"]
[]
[1,"裁判评分器","型号或规格：平板电脑（安装满足世界泳联花样游泳2022-2025规则操作终端）\n技术要求：评分裁判、难度技术控制员、同步控制员使用","台",20,"租赁"]
[2,"评分控制系统","型号或规格：满足花样游泳2022-2025规则专业竞赛评分控制系统；与评分控制器实时通讯\n技术要求：报名报项管理：手动添加运动员，通过文件导入的方式批量添加运动员\n现场编排：包含抽签编排和比赛安排两部分。能自动抽签或者手动录入签位，生成出场顺序信息，能够根据比赛结果自动晋级或者手动晋级。根据预赛成绩手动修改或自动生成决赛分组信息\n数据录入：读取计时记分设备数据或手动输入成绩等\n成绩报告输出：现场打印日程、成绩、最终排名等报表","套",1,"租赁"]
[3,"大屏显示接口系统","型号或规格：实时接收比赛数据，并显示更新在大屏幕上\n技术要求：实时将比赛成绩信息、成绩录取信息、颁奖信息等有效地展示在公共大屏上，提供多个可切换画面模板","套",1,"租赁"]
[4,"竞赛信息发布接口系统","型号或规格：生成ODF协议与竞赛综合发布系统，电视字幕，竞赛视频系统等信息对接\n技术要求：通过ODF协议与竞赛注册系统，综合发布系统进行无缝对接，接受报名报项数据，发布比赛日程，出场秩序，实时成绩，名次信息等","套",1,"租赁"]
[5,"主裁信息显示终端","型号或规格：双核/4G\n技术要求：显示比赛日程，比赛秩序信息，实时显示判评分信息","台",1,"租赁"]
[6,"副主裁信息显示终端","型号或规格：双核/4G\n技术要求：显示比赛日程，比赛秩序信息，实时显示判评分信息","台",1,"租赁"]
[7,"播音员信息显示终端","型号或规格：双核/4G\n技术要求：显示竞赛播音播报信息","台",1,"租赁"]
[8,"打印机","型号或规格：激光/A4\n用途：打印竞赛成绩报表","台",1,"租赁"]
[]
["二、通用器材清单"]
["序号","器材名称","功能与规格及说明","单位","数量","形式"]
[]
[1,"表演台","长15m×宽5m×高0.6m（不可有钉子）","个",1,"搭建（属临建、定制类）-租赁"]
[2,"表演台台阶","每阶20公分高×2m长×台阶面宽30公分（目前比赛运动员从表演台中间后面入场（左右均可），需要2个台阶，比赛结束从表演台一侧退场也需要台阶）","个",4,"搭建（属临建、定制类）-租赁"]
[3,"裁判台","长20m×宽2.5m×高0.6m","个",2,"搭建（属临建、定制类）-租赁"]
[4,"表演台、裁判台地毯","尺寸同表演台和裁判台（厚度1公分）","块",3,"搭建（属临建、定制类）-租赁"]
[5,"电线盖板","保护场内电源线（根据实际需求准备）","批",1,"租赁"]
[6,"电线插板滚轴","池边用（防水）","块",2,"租赁"]
[7,"竞赛桌子","裁判台上1米桌30张；其他用1.2米桌20张，","张",50,"租赁"]
[8,"竞赛椅子","竞赛用","个",65,"租赁"]
[9,"检录条凳","运动员用（1.5m）","个",10,"租赁"]
[10,"录像回放电视机","技术申诉录像回放（可以用电脑代替）\n（配连接线）","台",1,"租赁"]
[11,"成绩公告牌","竞赛用","块",1,"搭建（属临建、定制类）-租赁"]
[12,"乒乓球","比赛抽签用（尽量纯色），根据实际需求准备","个",200,"购买"]
[13,"透明储物盒(带盖）","比赛抽签用（31.5cm×21.5cm×高15cm）","个",2,"租赁"]
[14,"发令口哨","裁判长用","个",4,"购买"]
[15,"秒表","比赛计时用（考虑备用数量）","个",8,"购买"]
[16,"计算器","比赛用","个",4,"购买"]
[17,"记录板（夹板）","比赛记录用","个",25,"租赁"]
[18,"拉链袋","竞赛用","个",50,"购买"]
[19,"透明文件袋","竞赛用","个",50,"购买"]
[20,"笔记本","比赛记录用","本",50,"购买"]
[21,"签字笔","竞赛用（黑色）","支",80,"购买"]
[22,"剪刀","竞赛用","把",5,"购买"]
[23,"卷笔刀","竞赛用","个",2,"购买"]
[24,"订书机","竞赛用","个",4,"购买"]
[25,"回形针","竞赛用","盒",30,"购买"]
[26,"彩色复印纸A4","竞赛用（4种颜色各一箱）粉、黄、绿、蓝","箱",4,"购买"]
[27,"A4复印纸","竞赛用（白色）","箱",4,"购买"]
[28,"油性记号笔","竞赛用(黑色)","支",4,"购买"]
[29,"带橡皮头的铅笔","竞赛用","支",20,"购买"]
[30,"双面胶","竞赛用","卷",3,"购买"]
[31,"铡刀","竞赛用","个",2,"购买"]
[32,"电池","竞赛用（5号20节、7号10节）","节",50,"购买"]
[33,"胶水","竞赛用","个",2,"购买"]
[34,"快干胶棒","竞赛用","个",10,"购买"]
[35,"长尾夹","竞赛用（大30、中50、小60）","批",1,"购买"]
[36,"便签贴（5×5CM）","竞赛用","本",5,"购买"]
[37,"姓名贴","竞赛用","包",2,"购买"]
[38,"整理箱","竞赛用（约长50cm×宽40cm×高30cm）","个",20,"租赁"]
[39,"透明胶带","竞赛用","卷",3,"购买"]
[40,"裁纸刀","竞赛用","把",5,"购买"]
[41,"U盘","竞赛用（16G）","个",2,"购买"]
[42,"移动硬盘","保存比赛视频资料用（2T）","个",1,"购买（需提交至组委会）"]
[43,"插线板","（5个5m长，5个10m长）","个",10,"购买"]
[44,"扑克牌","上场裁判抽签用","副",5,"购买"]
[45,"电视","新闻发布厅（2台）、检录处、中心办公室、贵宾休息室、裁判员室和技术控制员室，需要配电脑连接线","台",7,"租赁"]
[46,"隔离带","场地内使用","批",1,"购买"]
[47,"裁判台围挡或桌布","按照两边裁判台上1m桌各15张和台下1.2m桌尺寸定制","批",1,"搭建（属临建、定制类）-租赁"]
[48,"大浴巾","竞赛用纯色浴巾160cm×90cm（救生围挡）","块",8,"购买"]
[49,"冰袋或冰块","运动员外敷（放冰桶内）","批",2,"购买冰袋"]
[50,"表演台干燥器",null,"批",1,"租赁"]
[51,"带锁的柜子","存放竞赛物品及技术官员个人物品","个",4,"租赁"]
[52,"绿植（鲜花）","表演台装饰使用","批",1,"租赁"]
[53,"运动员候分区沙发","白色沙发\n（四人位，防水皮质）","张",1,"租赁"]
[54,"颁奖花束（鲜花）","按获奖运动员人数准备","批",1,"购买"]
[55,"颁奖台","可站下10×3=30人","套",1,"搭建（属临建、定制类）-租赁"]
[56,"防滑垫","更衣室、比赛场地内","批",1,"租赁"]
[57,"笔记本电脑","竞赛用（要连接网络）","台",2,"租赁"]
[58,"台式电脑+打印机","竞赛用（要连接网络）","套",3,"租赁"]
[59,"一体打印机","竞赛办公室（打印机中至少有1台可彩打）","台",1,"租赁"]
[60,"速印机","复印成绩公告","台",1,"租赁"]
[61,"奖状打印机","竞赛用","台",2,"租赁"]
[62,"抽签箱","比赛用（25cm×25cm、中间圆孔10cm口径能放一只手进箱拿球、六面logo全覆盖）KT板","个",2,"租赁"]
[63,"打印机墨盒","竞赛用（按机型备用）","个",1,"租赁"]
[64,"场馆通讯手台","（配耳机及充电器）","个",10,"搭建（属临建、定制类）-租赁"]
[65,"救护车","需配有紧急处理的药品","台",1,"租赁"]
[66,"碎纸机",null,"台",1,"租赁"]